
CM620 Terminal Use


1. Overview

1.1 Software interface

The main interface includes a device information display area, a setting parameter area, and a debugging mode area.




Voltage calibration interface.




1. Software use

2.1 Connect the device


Just click the Connect device button, and the sending and receiving content can be displayed in the text box of the Debug mode area.






2.2 Start task


When the Balance port is set to True, the Balance of the battery must be connected. Cells can be set to Auto, which means that Cells are automatically obtained. If you choose false, you must select the corresponding Cells.



Only the current can be modified at the beginning of the mission.



2.3 Debug mode area can be manually input command debugging.



2.4 Voltage calibration can calibrate input voltage and output voltage. battery voltage.

